Instrument IQ for November/December 2016 – Answers

1. Yes, the straight-in approach is authorized (No PT 1400) and the descent should be initiated nine nautical miles (nm) back from the waypoint RW07 (MAP).

2. Not below 1,400 feet above sea level (ASL).

3. Yes, this runway is RVR equipped. Note the fact that RWY 07 is RVR equipped by referring to the advisory visibility on the ILS approach.

4. Yes, note “AN” and verify this by checking the Approach Lights Legend in the CAP GEN.

5. Hold as published at the HUH VOR, parallel entry.

6. 8; XX; NDB